PRODUKTVALGSPROGRAM FOR DUPLEX KOMPAKT ENHEDER 

BESKRIVELSE

Med produktvalgsprogrammet kan der udarbejdes et komplet teknisk design af DUPLEX KOMPAKT seriens enheder med varmegenvinding for en konkret brugssammenhæng. Programmet gør det muligt at vælge de enkelte enheder, inklusive varmeflader og køleflader, til et konkret anlæg ud fra detaljerede specifikationer.
Produktvalgsprogrammet kan levere en komplet teknisk rapport med alle tegninger, diagrammer, elektriske lednings-diagrammer samt et pris- og omkostningsoverslag baseret på de valgte enheder. Programmet understøtter konvertering af data til AutoCAD’s DXF-format, og til RTF og DOC-formaterne i WORD. Desuden kan en teknisk rapport konverteres til Acrobat’s PDF-format.

ÆNDRINGER SIDEN SENESTE VERSION

29.1.2025 ______ 9.50
- built-in electric preheaters and reheaters added also for semicompact units Multi (Eco)(-N), Roto (-N), Basic (-N)
- water preheaters PT added for semicompact units Multi (Eco)(-N), Basic (-N)
- external pressure on ODA and EHA plus air volume reserve for network leakage can now be entered in SMART boxes
- air volume from the hoods is now transferred automatically to the heat recovery unit, including a detailed table
- aMotion control system added also for kitchen ventilation
- further speedup of the program, including its installation
- update of the module for synergy with the Revit program - addition of 2025 Revit version support
- catalog sheet update
- other minor modifications and error corrections

14.6.2024 ______ 9.45
- new filtration class ePM1 80% (F9) added for DUPLEX units
- extended range of the rotary heat exchangers for DUPLEX Roto units
- new aM-XK4 expander for aMotion control system added for kitchen ventilation
- faster speed of the most parts of the program
- catalog sheet update
- other minor modifications and error corrections

11.1.2024 ______ 9.40
- added new small domestic ventilation unit DUPLEX Slim; unit is characterized by high compactness and excellent acoustic performance, to be mounted vertically
- catalogue sheet and certificates update
- other minor modifications and error corrections

11.10.2023 ______ 9.36
- added new generation of small domestic ventilation units DUPLEX Easy2; units are characterized by high compactness and excellent acoustic performance
- catalogue sheet and certificates update
- other minor modifications and error corrections

29.06.2023 ______ 9.35
- added smaller size of the DUPLEX Inter-H 770 under-ceiling decentral unit
- added new generation of small domestic ventilation units DUPLEX Pro and DUPLEX Pro-V; units meet the highest energy class A+ and are characterized by high compactness and excellent acoustic performance
- catalogue sheet and certificates update
- other minor modifications and error corrections

14.02.2023 ______ 9.31
- new line of decentralized units DUPLEX Inter-H added - special silent indoor units designed foremost for classrooms - ceiling-suspended type
- catalogue sheet and certificates update
- other minor modifications and error corrections

14.10.2022 ______ 9.30
- catalogue sheet and certificates update
- other minor modifications and error corrections

28.06.2022 ______ 9.25
- full support of the new, modern aMotion control system for DUPLEX Multi, MultiEco, Roto, Basic, EC5, ECV5 and Inter series units - the new control system is based on the successful RD5 control system and significantly expands control options, support for the new aTouch controllers (color touch screen) and the aDot (simpler variant)
- update of the module for synergy with the Revit program - addition of 2023 Revit version support
- catalogue sheet and certificates update
- other minor modifications and error corrections

10.02.2022 ______ 9.20
- a new (third) generation of DUPLEX Flexi units added - the new design "6v1" provides for all types of free-standing, ceiling-suspended and rooftop installation
- the section of ventilation calculation in (industrial) kitchens further expanded
- catalogue sheet and certificates update
- other minor modifications and error corrections

15.10.2021 ______ 9.10
- extended export for BIM (Revit) - it is now possible to export directly into RFA format
- the new section for (industrial) kitchen design calculation extended - calculations added, appliances added, kitchen hood design options extended 
- new units DUPLEX EC5-E and ECV5-E with enthalpy heat recovery core added
- update of the module for synergy with the Revit program - addition of 2022 Revit version support
- catalogue sheet and certificates update
- other minor modifications and error corrections

30.01.2021 ______ 9.00
- enhancement of new software feature for calculating the ventilation of (industrial) kitchens
- catalogue sheet and certificates update
- other minor modifications and error corrections

14.11.2020 ______ 8.98
- brand new range of path-breaking units DUPLEX RS5 for circulation ventilation, heating and cooling; suitable not only for commercial premises
- brand new range of units DUPLEX Flexi-V  (500-3500 m3/h)
- update of the module for synergy with the Revit program - addition of 2021 Revit version support
- brand new software feature for calculating the ventilation of (industrial) kitchens - the first released part involves the calculation of air volume based on the appliances installed, calculations according to the German guideline VDI 2052 and the new European norm EN 16282 are supported
- catalogue sheet update
- other minor modifications and error corrections

14.02.2020 ______ 8.97
- facelift of units DUPLEX RDH5-L - new generation of these special units for swimming pools are also suitable for saltwater pools
- accessories added (condensate pumps, motion sensor, external flaps for small ventilation units, etc.)
- catalogue sheet update
- other minor modifications and error corrections

15.11.2019 ______ 8.95
- catalogue sheet update
- other minor modifications and error corrections

15.02.2019 ______ 8.90
- new line of DUPLEX Silent units added - special line of units intended foremost for apartment buildings, ideally in combination with VAV boxes of the line SMART box and EASY box
- new line of decentralized units DUPLEX Inter added - special silent indoor units designed foremost for classrooms and offices
- added a new DUPLEX 650 Flexi, an all-purpose compact unit with very high heat recovery efficiency and versatile installation position
- catalogue sheet update
- other minor modifications and error corrections

30.09.2018 ______ 8.85
- support of R32 applications for DX coils
- built-in electric pre-heaters for roof-top units DUPLEX Multi-N, DUPLEX Multi Eco-N and DUPLEX Basic-N added
- full support of BIM added
a) selection software exports the selected units in the IFC format including all technical data (weight, airflow, pressure, efficiency, power input etc.) with active connectors to connect all ducts and media;
b) if the software Autodesk Revit is present, the option of importing IFC file is added here automatically; a direct two-way interface of the selection software and the Revit software is added too.
- catalogue sheet update
- other minor modifications and error corrections

28.03.2018 ______ 8.80
- full support of EASY boxes added - simple and versatile regulation boxes for VAV and CAV systems
- catalogue sheet update
- error corrections

28.11.2017 ______ 8.71
- catalogue sheet update
- error corrections

11.10.2017 ______ 8.70
- full support for SMART boxes added - a unique comprehensive central ventilation system combining VAV flow rate controllers and all-purpose heat recovery DUPLEX units - selection software makes it possible to add a SMART box with all details to each DUPLEX unit, calculates the total flow rate of the unit taking current factors into account, draws connection schematics etc.
- a new built-in electric reheaters for DUPLEX Multi, DUPLEX Multi Eco and DUPLEX Basic units added
- improved print and PDF export
- a new welcome window added
- catalogue sheet update
- other minor modifications and error corrections

15.02.2017 ______ version 8.50
- new units DUPLEX Multi 10.000 and 11.000, DUPLEX MultiEco 7.500 and 9.000, DUPLEX Basic 12.100 and 15.100 for rooftop as well as indoor installation added; the units can be fitted with the new RD5 control system with Internet access
- new control system CPM as an optional feature for DUPLEX Multi, MultiEco, Basic and Flexi units added; the new generation is based on the proven CPA control system with simple touch-screen display, newly also for use with chilled-water or direct cooling
- catalogue sheet update
- other minor modifications and error corrections

30.06.2016 ______ version 8.20
- added a brand new range of all-purpose ventilation units DUPLEX Roto size 1500, 2500, 4000 and 5000 for indoor (DUPLEX Roto) as well as rooftop (DUPLEX Roto-N) installation; the units can be fitted with the new RD5 control system with internet access
 - a new, fifth generation of ventilation units with air circulation DUPLEX RA5, RB5 and RK5 series added – each contains integrated new control system RD5 incl. internet access, while the new generation has significantly improved acoustic properties 
 - a new, fifth generation of DUPLEX RDH5 for ventilating small swimming pool areas added, incl. ventilation calculation according to swimming pool parameters
- catalogue sheet update
- other minor modifications and error corrections

31.03.2016 ______ version 8.10
- a new generation of small ventilation units DUPLEX EC5 and DUPLEX ECV5 added; the units have the new RD5 control system with Internet connection (high-comfort version) or the basic CPA control system (simple low-cost version); the newly designed units meet the requirements of the highest energy class A+ and have excellent noise parameters 
- many internal changes for faster program performance
- catalog sheet update
- other minor modifications and error corrections

19.01.2016 ______ version 8.00
- calculations and mandatory information under Ecodesign added – according Regulations 1253/2014 and 1254/2014
- an option to choose additional operating point for all units
- Windows 10 functionality optimization
- new generation of DUPLEX Flexi-D units added – all parameters are significantly improved as a result of new fans and modified heat recovery exchangers
- catalogue sheet update
- other minor modifications and error corrections

22.01.2015 ______ version 7.70
- added a new line DUPLEX Flexi-D – sizes 1000, 1500, 2500, 3500, an all-purpose compact unit with very high heat recovery efficiency and versatile installation position
- catalogue sheet update
- other minor modifications and error corrections

PROGRAM UPDATE IS PROVIDED BY

  ATREA s.r.o.
  Ceskoslovenske armady 32
  Jablonec nad Nisou
  466 05
  Czech Republic
  Phone: (+420) 483 368 111
  e-mail: atrea@atrea.cz 
  www.atrea.cz 

(c) 1998-2025 ATREA